set\_property PACKAGE\_PIN Y18 [get\_ports clk]

set\_property IOSTANDARD LVCMOS33 [get\_ports clk]

set\_property IOSTANDARD LVCMOS33 [get\_ports rst\_n]

set\_property IOSTANDARD LVCMOS33 [get\_ports sw0]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[15]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[14]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[13]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[12]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[11]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[10]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[9]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[8]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[7]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[6]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[5]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[4]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[3]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[2]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[1]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {led[0]}]

set\_property PACKAGE\_PIN W4 [get\_ports sw0]

set\_property PACKAGE\_PIN R4 [get\_ports rst\_n]

set\_property PACKAGE\_PIN N19 [get\_ports {led[0]}]

set\_property PACKAGE\_PIN N20 [get\_ports {led[1]}]

set\_property PACKAGE\_PIN M20 [get\_ports {led[2]}]

set\_property PACKAGE\_PIN K13 [get\_ports {led[3]}]

set\_property PACKAGE\_PIN K14 [get\_ports {led[4]}]

set\_property PACKAGE\_PIN M13 [get\_ports {led[5]}]

set\_property PACKAGE\_PIN L13 [get\_ports {led[6]}]

set\_property PACKAGE\_PIN K17 [get\_ports {led[7]}]

set\_property PACKAGE\_PIN J17 [get\_ports {led[8]}]

set\_property PACKAGE\_PIN L14 [get\_ports {led[9]}]

set\_property PACKAGE\_PIN L15 [get\_ports {led[10]}]

set\_property PACKAGE\_PIN L16 [get\_ports {led[11]}]

set\_property PACKAGE\_PIN K16 [get\_ports {led[12]}]

set\_property PACKAGE\_PIN M15 [get\_ports {led[13]}]

set\_property PACKAGE\_PIN M16 [get\_ports {led[14]}]

set\_property PACKAGE\_PIN M17 [get\_ports {led[15]}]