set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard\_val[5]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard\_val[4]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard\_val[3]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard\_val[2]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard\_val[1]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard\_val[0]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports i\_clk]

set\_property PACKAGE\_PIN Y18 [get\_ports i\_clk]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard[3]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard[2]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard[1]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard[0]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard[7]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard[6]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard[5]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard[4]}]

set\_property PACKAGE\_PIN A18 [get\_ports {keyboard[7]}]

set\_property PACKAGE\_PIN A20 [get\_ports {keyboard[6]}]

set\_property PACKAGE\_PIN B20 [get\_ports {keyboard[5]}]

set\_property PACKAGE\_PIN E18 [get\_ports {keyboard[4]}]

set\_property PACKAGE\_PIN F18 [get\_ports {keyboard[3]}]

set\_property PACKAGE\_PIN D19 [get\_ports {keyboard[2]}]

set\_property PACKAGE\_PIN E19 [get\_ports {keyboard[1]}]

set\_property PACKAGE\_PIN C19 [get\_ports {keyboard[0]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard\_val[6]}]

set\_property IOSTANDARD LVCMOS33 [get\_ports i\_rst\_n]

set\_property IOSTANDARD LVCMOS33 [get\_ports pause]

set\_property PACKAGE\_PIN R4 [get\_ports i\_rst\_n]

set\_property PACKAGE\_PIN W4 [get\_ports pause]

set\_property IOSTANDARD LVCMOS33 [get\_ports {keyboard\_val[7]}]

set\_property PACKAGE\_PIN F15 [get\_ports {keyboard\_val[7]}]

set\_property PACKAGE\_PIN C15 [get\_ports {keyboard\_val[0]}]

set\_property PACKAGE\_PIN C14 [get\_ports {keyboard\_val[1]}]

set\_property PACKAGE\_PIN E17 [get\_ports {keyboard\_val[2]}]

set\_property PACKAGE\_PIN F16 [get\_ports {keyboard\_val[3]}]

set\_property PACKAGE\_PIN F14 [get\_ports {keyboard\_val[4]}]

set\_property PACKAGE\_PIN F13 [get\_ports {keyboard\_val[5]}]

set\_property PACKAGE\_PIN F15 [get\_ports {keyboard\_val[6]}]